**Tender for Plastering, Painting, Tile-laying, the Manufacture, Supply, Delivery and Installation of Aluminum Apertures, and a Garage Door, Joinery/Woodworks (Internal Timber Doors And Fire Doors), and a Spiral Staircase as part of ERDF Project ERDF.05.121 – Wildlife Rehabilitation Centre**

**ERDF.05.0121 – Tender 009**

## TENDERER’S TECHNICAL OFFER (Note 3)

***N.B. The Key Experts Form (including Self-declaration form for Key Experts and the Statement re Exclusivity and Availability) are under Note 2A whereas the Literature is under Note 2B. Any other components of the technical offer are under Note 3.***

In response to Section 1, Article 7 (C) (i), Prospective bidders are requested to submit a Technical Offer in response to the specifications outlined in Section 4 of the Same tender Document. This shall include a method statement about how the bidder intends to carry out the works. In this regard, bidders are invited to use the present document to provide the required information, and serve as a checklist of all the documents they intend to submit. Without prejudice, nothing precludes bidders from using an alternative document, provided all the information requested below is provided. However, the submission shall be in a structured form and is to be in the same sequence as provided for ease of reference and evaluation

# NB – All supporting documents necessary (including the manufacturer’s Technical Literature) are listed in the Literature List. Bidders are advised to submit any Technical Literature with the offer.

# 1. Response to Section 4 of the tender Document

**Bidders shall fill in the table below**

| **Item No.** | **Description** | **Reference in Technical Specifications** | **Bidders are to insert the Manufacturer / Brand of the items being offered (as part of their technical offer Note 3).**  **These are to be inserted next to each item in the space provided below.** | **Bidders are to insert the Model / Catalogue No of the items being offered  (as part of their technical offer Note 3).**  **These are to be inserted next to each item in the space provided below.** |
| --- | --- | --- | --- | --- |
| **1** | Mortar for plastering and rendering | Subsection 4.3, Clause 1.2.1 |  |  |
| **2** | Paint to be used for internal spaces | Subsection 4.4, Clause 1.4.2. and 1.3 (GG Criteria) |  |  |
| **3** | Paint to be used for external spaces | Subsection 4.4, Clause 1.4.3. and 1.3 (GG Criteria) |  |  |
| **4** | Gres ceramic floor tiles for wet areas, bathrooms and kitchenettes | Subsection 4.5, of which 1.25 relates to GPP Criteria |  |  |
| **5** | Gres ceramic wall tiles for wet areas, bathrooms and kitchenettes | Subsection 4.5, of which 1.25 relates to GPP Criteria |  |  |
| **6** | Epoxy Resin Flooring | Subsection 4.5. |  |  |
| **7** | Aluminium apertures, including insulating material | Subsection 4.7, Article 1.2 of  which 1.2.3 relates to GPP Criteria |  |  |
| **8** | Garage door | Subsection 4.7, Article 1.3. |  |  |
| **9** | Timber laminated doors | Subsection 4.7, Article 1.4 |  |  |
| **10** | Fire-rated doors | Subsection 4.7, Article 1.4 |  |  |
| **11** | Spiral Staircase, including step | Subsection 4.8. |  |  |

# 2. Declarations

## Green Public Procurement Technical Specification Verifications – Declaration

### Explanatory Note

The declaration below refers to the Green Public Procurement (GPP) Technical Specifications Verifications found in the Technical Specifications, which the Economic Operator must comply with. It should be noted that the obligations specified in the declarations shall also be binding at execution stage. Non submission of such a declaration will result in the bid not being considered any further.

### Declaration

I declare that all products/materials used and proposed as part of the technical offer/questionnaire being submitted from this end, are in line with all GPP requirements and due verification/certification of this shall be provided during adjudication stage, if/when requested. Furthermore if I am the successful bidder, following signature of contract, I shall fulfil all the requirements specified as verification of compliance with the Green Public Procurement Technical Specifications, also during the implementation of the Contract.

|  |  |
| --- | --- |
| **Name**: |  |
| **Signature**: |  |
| **Date**: |  |

## Declaration by the Bidder concerning Technical Specifications

### Explanatory Note

Through the declaration below the economic operator will confirm abidance with all specifications in the tender document. Non submission of such a declaration will result in the bid not being considered any further.

### Declaration

I/We, the undersigned, hereby declare that I/We shall be abiding by the Technical Specifications in the Tender Document and that I shall be substantiating the offer as submitted, through the required documents as specified in the Tender document.

|  |  |
| --- | --- |
| **Name**: |  |
| **Signature**: |  |
| **Date**: |  |

## Declaration by the Bidder concerning warranty/guarantee

### Explanatory Note

The tender document requests bidders to provide a two-year warranty in line with EU legislation. Through this declaration, which explicitly recalls the terms of the tender document, the bidder is confirming such a declaration. Non submission of such a declaration will result in the bid not being considered any further.

### Declaration

I/We, the Undersigned, duly authorised to represent \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, hereby confirm that this bidder is providing a warranty, inclusive of parts and labour, for two\* years for as follows:

1. all external aluminium doors
2. all external aluminium windows
3. garage door
4. all internal doors and fire-rated doors
5. Spiral Staircase

\*Bidder MAY opt to increase such a warranty beyond the indicated minima.

This Guarantee/Warranty forms an integral part of the Contract entered into by the Contractor and the Contracting Authority for the implementation of the tender in caption.

|  |  |
| --- | --- |
| **Name**: |  |
| **Signature**: |  |
| **Date**: |  |

# 3. Gantt Chart

The Bidder is to fill in the following Gantt Chart to indicate when and how each activity is to be carried out. Within the five month period allowed as Execution of the Contract as per Special Conditions. Bidders are asked to indicate sub-tasks as necessary. The Gantt Chart is split in Weeks, and covers 26-weeks

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | **Weeks** | | | | | | | | | | | | | | | | | | | | | | | | | |
|  | **1** | **2** | **3** | **4** | **5** | **6** | **7** | **8** | **9** | **10** | **11** | **12** | **13** | **14** | **15** | **16** | **17** | **18** | **19** | **20** | **21** | **22** | **Comments** | | | |
| **Excavation and Clearing Works** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | | |
| Remove floor finishes, steel elements |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | | |
| Demolish existing reinforced concrete slabs and beams |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Trimming of any existing dead concrete surface |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Demolish existing ramp |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Preparation for the aviary ground slab. |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Preparation for the ground slab next to outbuildings. |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Dismantling of limestone masonry |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Demolish concrete slabs in outbuildings |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Connection with Sewage treatment plant – trenching of road, lay pipes, infilling, asphalting. |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Connection with Sewage treatment plant – trenching in concrete slab, lay pipes, infilling. |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Connection with Sewage treatment plant and sleeves for M&Es – trenching in ground, lay pipes, infilling. |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Repair, testing, investigation** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | | |
| Clean existing concrete surfaces, treat exposed steel reinforcement |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | | |
| GPR testing |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Sampling of concrete cores |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Install strengthening steel mesh and grout |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Concrete and steel works** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | | |
| Casting of cast-in situ concrete blinding |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | | |
| Steel reinforcement for concrete ground slab and suspended slabs. |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Casting of cast-in situ concrete ground slabs |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Casting of cast-in situ concrete suspended slabs |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Casting of cast-in situ concrete suspended beams |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Casting of cast-in situ concrete topping on prestressed precast slabs |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Casting of water spouts |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Cast roof screed laid to falls |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Prestressed Concrete Planks** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Lay precast prestressed concrete slabs |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Masonry stone** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Construction of limestone masonry stone blockwork, bedded, jointed and pointed |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Formation of doors and/or windows within existing masonry skin fabric. |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Construction of 230mm thick hollow concrete blockwork, bedded, jointed and pointed. |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Infill of 230mm thick HCB with C20 concrete |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Other Items** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Cleaning of concrete, apply primer and tar as waterproofing |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Supply and lay of torch welded bituminious waterproofing membrane |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Supply, laying and compacting of Type 1 material |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Supply and installation of expanded polystyrene (jablo) insulation panels on roof |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Supply and installation of lightpipes |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| The cutting of 10mm width and 25mm in depth chase within roof screed and fill with mastic sealant and foam rod. |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Drainage works |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Plumbing Works |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Supply, laying and compacting of graded fill material |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

# 4. Checklist of documents to be provided

|  |  |
| --- | --- |
| Tender Form and Tenderer’s Declaration |  |
| Technical offer (Including GPP declaration and Self declaration form) |  |
| Financial Bid Form |  |
| Statement on Conditions of Employment |  |
| Power of Attorney (if applicable) |  |
| Information re Joint Venture/Consortium |  |
| European Single Procurement Document (ESPD) |  |
| Key Experts Forms (including Statement of Exclusivity and Availability Form, and Self Declaration Form) |  |
| Literature (vide Literature List, includes proof re key Experts) |  |